,Suction Size##pipe_size##inches,Discharge Size##pipe_size##inches,Maximum Flow Rate Value##Number##General,Connection Type##other##,Voltage##electrical_potential##volts,Number of Poles##other##,Phase##other##,Frequency##electrical_frequency##hertz,Motor Power##electrical_power##horsepower,Motor Full Load Amps##electrical_current##amperes,Rated Speed (RPM)##other##,Unit Weight Value##number##general,Maximum Working Pressure##piping_pressure##pounds_force_per_square_inch,Maximum Operating Temperature##hvac_temperature##Fahrenheit,Minimum Operating Temperature##hvac_temperature##Fahrenheit,Description##other##,Model Number##other##,Part Number##other##,A##length##inches,B##length##inches,C##length##inches,D##length##inches,E##length##inches,F##length##inches,G##length##inches,Pump Housing Material##other##,Series##other##,URL##other##,Product Page URL##other##,Standards##other##
0.5in. Sweat_NBF-8S/LW,0.5,0.5,10,Sweat,115,1,1,60,0.05227882,0.38,2800,9,150,230,40,"In-line System Lubricated Circulating Pump, Lead-Free Bronze",NBF-8S/LW,103257LF,4.875,3.1875,0.5,5.21875,4.28125,5,2.5,Metal - B&G - LF Bronze,NBF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/nbf/,CSA certified to NSF/ANSI 372
0.5in. Sweat_NBF-10S/LW,0.5,0.5,10,Sweat,115,1,1,60,0.069705094,0.46,2800,9,150,230,40,"In-line System Lubricated Circulating Pump, Lead-Free Bronze",NBF-10S/LW,103259LF,4.875,3.1875,0.5,5.21875,4.28125,5,2.5,Metal - B&G - LF Bronze,NBF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/nbf/,CSA certified to NSF/ANSI 372
0.5in. Sweat_NBF-18S,0.5,0.5,10,Sweat,115,1,1,60,0.120643432,0.74,3000,9,150,230,40,"In-line System Lubricated Circulating Pump, Lead-Free Bronze",NBF-18S,103316LF,4.875,3.1875,0.5,5.21875,4.28125,5,2.5,Metal - B&G - LF Bronze,NBF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/nbf/,CSA certified to NSF/ANSI 372
