,Suction Size##pipe_size##inches,Discharge Size##pipe_size##inches,Maximum Flow Rate Value##Number##General,Connection Type##other##,Voltage##electrical_potential##volts,Number of Poles##other##,Phase##other##,Frequency##electrical_frequency##hertz,Motor Power##electrical_power##horsepower,Motor Full Load Amps##electrical_current##amperes,Rated Speed (RPM)##other##,Unit Weight Value##number##general,Maximum Working Pressure##piping_pressure##pounds_force_per_square_inch,Maximum Operating Temperature##hvac_temperature##Fahrenheit,Minimum Operating Temperature##hvac_temperature##Fahrenheit,Description##other##,Model Number##other##,Part Number##other##,A##length##inches,B##length##inches,C##length##inches,D##length##inches,E##length##inches,F##length##inches,G##length##inches,Pump Housing Material##other##,Series##other##,URL##other##,Product Page URL##other##,Standards##other##
0.75in. Flange_SSF-12F/LW,0.75,0.75,17,Flange,115,1,1,60,0.073726542,0.48,2800,9.5,150,230,40,"In-line System Lubricated Circulating Pump, Stainless Steel",SSF-12F/LW,103358LF,4.875,3.1875,3.1875,5.5625,3.6875,6.375,3.1875,Metal - B&G - Stainless Steel,SSF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/stainless-steel-ssf-22-ssf-12-ssf-9-circulator/,CSA certified to NSF/ANSI 372 
1in. Flange_SSF-12F/LW,1,1,17,Flange,115,1,1,60,0.073726542,0.48,2800,9.5,150,230,40,"In-line System Lubricated Circulating Pump, Stainless Steel",SSF-12F/LW,103358LF,4.875,3.1875,3.1875,5.5625,3.6875,6.375,3.1875,Metal - B&G - Stainless Steel,SSF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/stainless-steel-ssf-22-ssf-12-ssf-9-circulator/,CSA certified to NSF/ANSI 372 
1.25in. Flange_SSF-12F/LW,1.25,1.25,17,Flange,115,1,1,60,0.073726542,0.48,2800,9.5,150,230,40,"In-line System Lubricated Circulating Pump, Stainless Steel",SSF-12F/LW,103358LF,4.875,3.1875,3.1875,5.5625,3.6875,6.375,3.1875,Metal - B&G - Stainless Steel,SSF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/stainless-steel-ssf-22-ssf-12-ssf-9-circulator/,CSA certified to NSF/ANSI 372 
1.5in. Flange_SSF-12F/LW,1.5,1.5,17,Flange,115,1,1,60,0.073726542,0.48,2800,9.5,150,230,40,"In-line System Lubricated Circulating Pump, Stainless Steel",SSF-12F/LW,103358LF,4.875,3.1875,3.1875,5.5625,3.6875,6.375,3.1875,Metal - B&G - Stainless Steel,SSF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/stainless-steel-ssf-22-ssf-12-ssf-9-circulator/,CSA certified to NSF/ANSI 372 
0.75in. Flange_SSF-22,0.75,0.75,22,Flange,115,1,1,60,0.123324397,0.8,2940,9.5,150,230,40,"In-line System Lubricated Circulating Pump, Stainless Steel",SSF-22,103357LF,4.875,3.1875,3.1875,5.5625,3.6875,6.375,3.1875,Metal - B&G - Stainless Steel,SSF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/stainless-steel-ssf-22-ssf-12-ssf-9-circulator/,CSA certified to NSF/ANSI 372 
1in. Flange_SSF-22,1,1,22,Flange,115,1,1,60,0.123324397,0.8,2940,9.5,150,230,40,"In-line System Lubricated Circulating Pump, Stainless Steel",SSF-22,103357LF,4.875,3.1875,3.1875,5.5625,3.6875,6.375,3.1875,Metal - B&G - Stainless Steel,SSF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/stainless-steel-ssf-22-ssf-12-ssf-9-circulator/,CSA certified to NSF/ANSI 372 
1.25in. Flange_SSF-22,1.25,1.25,22,Flange,115,1,1,60,0.123324397,0.8,2940,9.5,150,230,40,"In-line System Lubricated Circulating Pump, Stainless Steel",SSF-22,103357LF,4.875,3.1875,3.1875,5.5625,3.6875,6.375,3.1875,Metal - B&G - Stainless Steel,SSF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/stainless-steel-ssf-22-ssf-12-ssf-9-circulator/,CSA certified to NSF/ANSI 372 
1.5in. Flange_SSF-22,1.5,1.5,22,Flange,115,1,1,60,0.123324397,0.8,2940,9.5,150,230,40,"In-line System Lubricated Circulating Pump, Stainless Steel",SSF-22,103357LF,4.875,3.1875,3.1875,5.5625,3.6875,6.375,3.1875,Metal - B&G - Stainless Steel,SSF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/stainless-steel-ssf-22-ssf-12-ssf-9-circulator/,CSA certified to NSF/ANSI 372 
