,Suction Size##pipe_size##inches,Discharge Size##pipe_size##inches,Connection Type##other##,Voltage##electrical_potential##volts,Number of Poles##other##,Phase##other##,Frequency##electrical_frequency##hertz,Motor Power##electrical_power##horsepower,Motor Full Load Amps##electrical_current##amperes,Rated Speed (RPM)##other##,Unit Weight Value##number##general,Maximum Working Pressure##piping_pressure##pounds_force_per_square_inch,Maximum Operating Temperature##hvac_temperature##Fahrenheit,Minimum Operating Temperature##hvac_temperature##Fahrenheit,Description##other##,Model Number##other##,Part Number##other##,A##length##inches,B##length##inches,C##length##inches,Overall Length##length##inches,Pump Housing Material##other##,Series##other##,URL##other##,Product Page URL##other##,Standards##other##
0.75in. Flange_LR-20WR,0.75,0.75,Flange,115,1,1,60,0.167560322,1.1,2950,10.4,150,225,0,"Low Head, In-line System Lubricated Circulating Pump, Cast Iron",LR-20WR,106507,6.375,4.25,3.875,6,Metal - B&G - Cast Iron - Red,LR,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/heating-cooling-circulators/low-head-circulators-lr-15bwr-lr-20wr/,"CSA certified to NSF/ANSI 372,  ISO-9001"
1in. Flange_LR-20WR,1,1,Flange,115,1,1,60,0.167560322,1.1,2950,10.4,150,225,0,"Low Head, In-line System Lubricated Circulating Pump, Cast Iron",LR-20WR,106507,6.375,4.25,3.875,6,Metal - B&G - Cast Iron - Red,LR,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/heating-cooling-circulators/low-head-circulators-lr-15bwr-lr-20wr/,"CSA certified to NSF/ANSI 372,  ISO-9001"
1.25in. Flange_LR-20WR,1.25,1.25,Flange,115,1,1,60,0.167560322,1.1,2950,10.4,150,225,0,"Low Head, In-line System Lubricated Circulating Pump, Cast Iron",LR-20WR,106507,6.375,4.25,3.875,6,Metal - B&G - Cast Iron - Red,LR,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/heating-cooling-circulators/low-head-circulators-lr-15bwr-lr-20wr/,"CSA certified to NSF/ANSI 372,  ISO-9001"
1.5in. Flange_LR-20WR,1.5,1.5,Flange,115,1,1,60,0.167560322,1.1,2950,10.4,150,225,0,"Low Head, In-line System Lubricated Circulating Pump, Cast Iron",LR-20WR,106507,6.375,4.25,3.875,6,Metal - B&G - Cast Iron - Red,LR,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/heating-cooling-circulators/low-head-circulators-lr-15bwr-lr-20wr/,"CSA certified to NSF/ANSI 372,  ISO-9001"
0.75in. Flange_LR-15BWR,0.75,0.75,Flange,115,1,1,60,0.167560322,1.1,2950,10.4,150,225,0,"Low Head, In-line System Lubricated Circulating Pump, Lead-Free Bronze",LR-15BWR,106514LF,6.375,4.25,3.875,6,Metal - B&G - LF Bronze,LR,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/heating-cooling-circulators/low-head-circulators-lr-15bwr-lr-20wr/,"CSA certified to NSF/ANSI 372,  ISO-9001"
1in. Flange_LR-15BWR,1,1,Flange,115,1,1,60,0.167560322,1.1,2950,10.4,150,225,0,"Low Head, In-line System Lubricated Circulating Pump, Lead-Free Bronze",LR-15BWR,106514LF,6.375,4.25,3.875,6,Metal - B&G - LF Bronze,LR,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/heating-cooling-circulators/low-head-circulators-lr-15bwr-lr-20wr/,"CSA certified to NSF/ANSI 372,  ISO-9001"
1.25in. Flange_LR-15BWR,1.25,1.25,Flange,115,1,1,60,0.167560322,1.1,2950,10.4,150,225,0,"Low Head, In-line System Lubricated Circulating Pump, Lead-Free Bronze",LR-15BWR,106514LF,6.375,4.25,3.875,6,Metal - B&G - LF Bronze,LR,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/heating-cooling-circulators/low-head-circulators-lr-15bwr-lr-20wr/,"CSA certified to NSF/ANSI 372,  ISO-9001"
1.5in. Flange_LR-15BWR,1.5,1.5,Flange,115,1,1,60,0.167560322,1.1,2950,10.4,150,225,0,"Low Head, In-line System Lubricated Circulating Pump, Lead-Free Bronze",LR-15BWR,106514LF,6.375,4.25,3.875,6,Metal - B&G - LF Bronze,LR,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/heating-cooling-circulators/low-head-circulators-lr-15bwr-lr-20wr/,"CSA certified to NSF/ANSI 372,  ISO-9001"
