,Suction Size##pipe_size##inches,Discharge Size##pipe_size##inches,Maximum Flow Rate Value##Number##General,Connection Type##other##,Voltage##electrical_potential##volts,Number of Poles##other##,Phase##other##,Frequency##electrical_frequency##hertz,Motor Power##electrical_power##horsepower,Motor Full Load Amps##electrical_current##amperes,Rated Speed (RPM)##other##,Unit Weight Value##number##general,Maximum Working Pressure##piping_pressure##pounds_force_per_square_inch,Maximum Operating Temperature##hvac_temperature##Fahrenheit,Minimum Operating Temperature##hvac_temperature##Fahrenheit,Description##other##,Model Number##other##,Part Number##other##,A##length##inches,B##length##inches,C##length##inches,D##length##inches,E##length##inches,F##length##inches,G##length##inches,Connection Type Selector##other##,Pump Housing Material##other##,Series##other##,URL##other##,Product Page URL##other##,Standards##other##
0.5in. Sweat Union_NBF-9U/LW,0.5,0.5,12,Sweat Union,115,1,1,60,0.054959786,0.4,2800,9.3,150,230,40,"In-line System Lubricated Circulating Pump, Lead-Free Bronze",NBF-9U/LW,103258LF,4.875,3.1875,1.25,5.0625,3.6875,6.125,3.0625,1,Metal - B&G - LF Bronze,NBF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/nbf/,CSA certified to NSF/ANSI 372
0.75in. Sweat Union_NBF-9U/LW,0.75,0.75,12,Sweat Union,115,1,1,60,0.054959786,0.4,2800,9.3,150,230,40,"In-line System Lubricated Circulating Pump, Lead-Free Bronze",NBF-9U/LW,103258LF,4.875,3.1875,1.25,5.0625,3.6875,6.125,3.0625,2,Metal - B&G - LF Bronze,NBF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/nbf/,CSA certified to NSF/ANSI 372
0.75in. FNPT Union_NBF-9U/LW,0.75,0.75,12,FNPT Union,115,1,1,60,0.054959786,0.4,2800,9.3,150,230,40,"In-line System Lubricated Circulating Pump, Lead-Free Bronze",NBF-9U/LW,103258LF,4.875,3.1875,1.25,5.0625,3.6875,6.125,3.0625,3,Metal - B&G - LF Bronze,NBF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/nbf/,CSA certified to NSF/ANSI 372
0.5in. Sweat Union_NBF-12U/LW,0.5,0.5,17,Sweat Union,115,1,1,60,0.073726542,0.48,2800,9.3,150,230,40,"In-line System Lubricated Circulating Pump, Lead-Free Bronze",NBF-12U/LW,103261LF,4.875,3.1875,1.25,5.0625,3.6875,6.125,3.0625,1,Metal - B&G - LF Bronze,NBF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/nbf/,CSA certified to NSF/ANSI 372
0.75in. Sweat Union_NBF-12U/LW,0.75,0.75,17,Sweat Union,115,1,1,60,0.073726542,0.48,2800,9.3,150,230,40,"In-line System Lubricated Circulating Pump, Lead-Free Bronze",NBF-12U/LW,103261LF,4.875,3.1875,1.25,5.0625,3.6875,6.125,3.0625,2,Metal - B&G - LF Bronze,NBF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/nbf/,CSA certified to NSF/ANSI 372
0.75in. FNPT Union_NBF-12U/LW,0.75,0.75,17,FNPT Union,115,1,1,60,0.073726542,0.48,2800,9.3,150,230,40,"In-line System Lubricated Circulating Pump, Lead-Free Bronze",NBF-12U/LW,103261LF,4.875,3.1875,1.25,5.0625,3.6875,6.125,3.0625,3,Metal - B&G - LF Bronze,NBF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/nbf/,CSA certified to NSF/ANSI 372
0.5in. Sweat Union_NBF-22U,0.5,0.5,22,Sweat Union,115,1,1,60,0.123324397,0.8,2940,9.3,150,230,40,"In-line System Lubricated Circulating Pump, Lead-Free Bronze",NBF-22U,103255LF,4.875,3.1875,1.25,5.0625,3.6875,6.125,3.0625,1,Metal - B&G - LF Bronze,NBF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/nbf/,CSA certified to NSF/ANSI 372
0.75in. Sweat Union_NBF-22U,0.75,0.75,22,Sweat Union,115,1,1,60,0.123324397,0.8,2940,9.3,150,230,40,"In-line System Lubricated Circulating Pump, Lead-Free Bronze",NBF-22U,103255LF,4.875,3.1875,1.25,5.0625,3.6875,6.125,3.0625,2,Metal - B&G - LF Bronze,NBF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/nbf/,CSA certified to NSF/ANSI 372
0.75in. FNPT Union_NBF-22U,0.75,0.75,22,FNPT Union,115,1,1,60,0.123324397,0.8,2940,9.3,150,230,40,"In-line System Lubricated Circulating Pump, Lead-Free Bronze",NBF-22U,103255LF,4.875,3.1875,1.25,5.0625,3.6875,6.125,3.0625,3,Metal - B&G - LF Bronze,NBF,https://www.xylem.com/en-us/,https://bellgossett.com/pumps-circulators/circulator-pumps/potable-water-circulators/nbf/,CSA certified to NSF/ANSI 372
